These are pure DOS drivers for the Creative Sound Blaster Live! cards.
They should work with most Live! cards, but I've tested them with SB0060, SB0100, CT4780 and CT4830.

They will work with a pure MS-DOS 6.22, 7.0 or 7.1 installation.

They will also work in MS-DOS mode of Windows 9x.

Run LIVESET.BAT once. This will make the card independent of Windows and programm its resources.
You can change the resources, by editing CTSYN.INI.

Run LIVEINIT.BAT after every boot to initialise the card. Just call it from AUTOEXEC.BAT if you like.

Run SBEMIXER.EXE to set the mixer levels.

I've also replaced the default 2MB SoundFont with the nicer 8MB once.
This will delay the driver initialisation a bit, so it can take like 10 seconds or so.

They should work with most, but I've tested them with SB0060, SB0100, CT4780 and CT4830.



I hope they work out for you!

Phil aka PhilsComputerLab
JAN 2018