Microsoft MS-DOS 2.00 [Xerox 820 16-8]
Released in 1984 by Xerox
For Xerox 820 16-8 computers only.

This is the version of MS-DOS required to operate a Xerox 820 16-8
computer. The Xerox 820 16-8 is a dual CPU system that contains both
a Z-80 for CP/M software and an 8086 CPU for MS-DOS. This machine was
notable as it could run both OSes at the same time. It is not IBM PC
hardware compatible, and will not run IBM PC-DOS or a generic MS-DOS.

This adaptation of MS-DOS will not run on an IBM PC, IBM PC clone, or
IBM PC emulators. It can only be used with a Xerox 820 16-8 computer.
(Earlier Xerox 820 models did not have the 8086).

Archive includes two 5.25" 360k floppy disk images.

The ImageDisk files should be used to create a new disk, as the 
disks appear to have an odd interleave. (The SuperCard Pro source 
dumps are included for completeness).
